For 1990-2009 cars

# REAR COMPARTMENT LID DOES NOT STAY OPEN

#### SUBJECT: REAR COMPARTMENT LID DOES NOT STAY OPEN (ADJUST TORQUE RODS)

#### MODELS: 1994-95 OLDSMOBILE NINETY EIGHT WITH REAR COMPARTMENT LID TORQUE ROD SYSTEM

#### CONDITION:

SOME OWNERS MAY COMMENT THAT THE REAR COMPARTMENT LID MAY DRIFT DOWN WHEN THE VEHICLE IS PARKED ON AN INCLINE OR IF A STRONG WIND CATCHES THE LID.

#### CAUSE:

THE INITIAL SETTING OF THE REAR COMPARTMENT LID TORQUE RODS DOES NOT PROVIDE SUFFICIENT TENSION TO HOLD THE REAR COMPARTMENT LID IN THE OPEN POSITION.

#### CORRECTION:

ADJUST REAR COMPARTMENT LID TORQUE RODS USING TORQUE ROD ADJUSTMENT TOOL, J-41358-1, TO INCREASE TORQUE ROD OUTPUT. REFER TO FIGURE 1.

#### WARRANTY INFORMATION:

FOR VEHICLES REPAIRED UNDER WARRANTY, USE:

LABOR OPERATION NUMBER: B5463 (RIGHT) B5464 (LEFT) USE PUBLISHED LABOR OPERATION TIME.

FIGURES: 1 1. HINGE ASSEMBLY 2. TORQUE ROD 3. TOOL, J41358-1 4. RATCHET/BREAKER BAR 5. 10" EXTENSION

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.