For 1990-2009 cars

# SMU - SECTION 6A8 - REVISED OIL PAN SERVICE PROCEDURE

#### SUBJECT: SERVICE MANUAL UPDATE-SECTION 6A8-REVISED OIL PAN SERVICE PROCEDURE

#### MODELS: 1995 BUICK PARK AVENUE, RIVIERA 1995 CHEVROLET CAMARO 1995 OLDSMOBILE EIGHTY EIGHT, NINETY EIGHT 1995 PONTIAC BONNEVILLE, FIREBIRD WITH 3800 ENGINE (VIN K - RPO L36)

THE FOLLOWING INFORMATION MUST BE FOLLOWED TO PREVENT DAMAGING THE OIL LEVEL SENSOR DURING REMOVAL OF THE OIL PAN AND BAFFLE.

#### NOTICE: THE OIL LEVEL SENSOR (LOCATED IN THE OIL PAN), MUST BE REMOVED BEFORE THE OIL PAN. IF THE OIL PAN AND BAFFLE ARE REMOVED FIRST, DAMAGE TO THE SENSOR MAY OCCUR WHEN THE BAFFLE CONTACTS THE SENSOR.

THE FOLLOWING INFORMATION MUST BE FOLLOWED TO PREVENT DAMAGING THE OIL LEVEL SENSOR DURING INSTALLATION OF THE OIL PAN AND BAFFLE.

#### NOTICE: THE OIL LEVEL SENSOR (LOCATED IN THE OIL PAN), MUST BE INSTALLED AFTER THE OIL PAN AND BAFFLE. IF THE OIL LEVEL SENSOR IS INSTALLED FIRST, DAMAGE TO THE SENSOR MAY OCCUR WHEN THE BAFFLE CONTACTS THE SENSOR.

FIGURES: 0 ATTACHMENTS: 0

GENERAL MOTORS BULLETINS ARE INTENDED FOR USE BY PROFESSIONAL TECHNICIANS, NOT A "DO-IT-YOURSELFER". THEY ARE WRITTEN TO INFORM THOSE TECHNICIANS OF CONDITIONS THAT MAY OCCUR ON SOME VEHICLES, OR TO PROVIDE INFORMATION THAT COULD ASSIST IN THE PROPER SERVICE OF A VEHICLE. PROPERLY TRAINED TECHNICIANS HAVE THE EQUIPMENT, TOOLS, SAFETY INSTRUCTIONS AND KNOW-HOW TO DO A JOB PROPERLY AND SAFELY. IF A CONDITION IS DESCRIBED, DO NOT ASSUME THAT THE BULLETIN APPLIES TO YOUR VEHICLE, OR THAT YOUR VEHICLE WILL HAVE THAT CONDITION. SEE A GENERAL MOTORS DEALER SERVICING YOUR BRAND OF GENERAL MOTORS VEHICLE FOR INFORMATION ON WHETHER YOUR VEHICLE MAY BENEFIT FROM THE INFORMATION.

COPYRIGHT 1995 GENERAL MOTORS CORPORATION. ALL RIGHTS RESERVED.