For 1990-2009 cars

Name | Location | Locator View | Connector End View | Group No.
--- | --- | --- | --- | ---
High Speed Cooling Fan Relay | Rear of the engine compartment, below the LH U/H fuse block | 8A-201-11 Fig 21 | -- | 1.055
IP Fuse Block | Behind the LH side of the steering column, behind the trim panel | 8A-201-23 Fig 43 | -- | --
LH Cooling Fan Motor | Front of the engine compartment | 8A-201-1 Fig 1 | -- | 1.055
LH Maxi® Fuse Block | LH rear of the engine compartment | 8A-201-11 Fig 21 | -- | --
Low Speed Cooling Fan Relay | Rear of the engine compartment, below the LH U/H fuse block | 8A-201-11 Fig 21 | -- | 1.055
Powertrain Control Module(PCM) | LH front of the engine compartment, near the evaporative emission (EVAP) canister | 8A-201-8 Fig 15 | -- | 3.670

• | C1 (80 cavities)

Engine harness to the PCM, LH front of the engine compartment, near the evaporative emission (EVAP) canister

--

6-Engine Controls

--

RH Cooling Fan Motor | Front of the engine compartment | 8A-201-1 Fig 1 | -- | 1.055
C101 (66 cavities) | RH rear of the engine compartment, near the A/C accumulator | 8A-201-28 Fig 53 | -- | --
G104 | LH front fender, near the air cleaner assembly | 8A-201-6 Fig 12 | -- | --
P100 | LH rear of the engine compartment, next to the LH strut tower | 8A-201-10 Fig 19 | -- | --
S104 | Body main harness, about 25 cm (9.8 in) from the cooling fan relay, Maxi® fuse block breakout | 8A-201-11 Fig 22 | -- | --
S124 | Body main harness, LH rear of the engine compartment | -- | -- | --
S128 | Body main harness, about 6.5 cm (2.6 in) from the cooling fan connector breakout | 8A-201-7 Fig 13 | -- | --