For 1990-2009 cars

## Valve Rocker Arm Cover Replacement Left

### Removal Procedure

1. Remove the left spark plug wire harness.
2. Remove the rocker arm cover bolts.
3. Remove the rocker arm cover.

### Installation Procedure

1. Install the rocker arm cover.
2. Apply thread lock compound or equivalent to the bolt threads.
3. Install the rocker arm cover bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Install the spark plug wire harness.

## Valve Rocker Arm Cover Replacement Right

### Removal Procedure

1. Remove the generator rear retaining brace.
2. Remove the spark plug wires.
3. Remove the rocker arm cover bolts.
4. Remove the rocker arm cover.

### Installation Procedure

1. Install the rocker arm cover.
2. Apply thread lock compound or equivalent to the bolt threads.
3. Install the rocker arm cover bolts.

Tighten
Tighten the bolts to 10 N·m (89 lb in).

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

4. Connect the spark plug wires.
5. Install the generator rear retaining brace.