For 1990-2009 cars

# BRUSH PACKAGE REPLACEMENT FOR WINDOW LIFT MOTORS

#### MODELS/YEARS 1988 NINETY-EIGHT, EIGHTY-EIGHT AND CUTLASS SUPREME MODELS

Some 1988 Ninety-Eight, Eighty-Eight and Cutlass Supreme models may exhibit power window lift motors that start out as intermittent operation and eventually become inoperative. This condition may be due to restricted brushes making intermittent contact with the armature commutator.

New brush replacement packages may be ordered from GMSPO and the part numbers are as follows:

22094719 - Ninety-Eight and Eighty-Eight

22094720 - Right Side Cutlass Supreme

22094721 - Left Side Cutlass Supreme

Parts are currently available from GMSPO.

An instruction sheet describing the proper procedures is included in each package. While regulator and motor removal from the door is required, IT IS NOT NECESSARY to remove the motor from the regulator to replace the brushes. It will be necessary to secure the regulator sector gear to the backplate prior to performing this repair.

#### WARRANTY INFORMATION:

Labor Operation Number: N3314 - Right Front

N3315 - Left Front

N3324 - Right Rear

N3325 - Left Rear

Labor Time: Use applicable times for styles involved.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.