For 1990-2009 cars

# SERV. MANUAL UPDATE - SEC. 6E3 REVISED A3 CHART (PAGE 1)

#### SUBJECT: SERVICE MANUAL UPDATE - SECTION 6E3 REVISED A3 CHART (PAGE 1)

#### VEHICLES AFFECTED: 1991 "C, E" AND 1992 "C, H" MODELS WITH 3.8L (VIN L)

This Bulletin updates Section 6E3, "Driveability and Emissions" Chart A3, "Engine Cranks But Won't Run" (Type I Ignition) (Page 1 of 4) for 1991 "C" and 1992 "C/H" models and Chart A3 (Page 1 of 3) for 1991 "E" models equipped with the 3800 (VIN L) engine.

The revised chart addresses the possibility of an invalid PASS-Key fuel enable signal causing the "Cranks But Won't Run" condition.

Pages affected are as follows:

- 1992 Pontiac "H" Page 6E3 - A-23 - 1992 Oldsmobile and Buick "C/H" Page 6E3 - A-25 - 1991 Oldsmobile and Buick "C" Page 6E3 - A-25 - 1991 Oldsmobile "E" Page 6E3 - A-25 - 1991 Buick "E" Page 6E3 - A-23

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.