For 1990-2009 cars

# CLUNKING NOISE IN FRT. SUSPEN. (REPL. STAB. SHAFT LINK ASSY.)

#### SUBJECT: CLUNKING NOISE IN FRONT SUSPENSION (REPLACE STABILIZER SHAFT LINK ----------------------------------------------------------------- ASSEMBLIES) -----------

#### VEHICLES AFFECTED: 1992-23 "C/H" SERIES --------------------

#### APPLICATION:

------------

1992-93 Buick Park Avenue with F41 suspension 1992-93 Buick Le Sabre with FE3 suspension 1992-93 Oldsmobile Ninety Eight with F41 suspension 1992-93 Oldsmobile Eighty Eight with FE3 suspension 1992-93 Pontiac Bonneville

#### CONDITION:

----------

Some vehicles may exhibit a clunking noise in the front suspension when driving over bumps. This condition is more noticeable in cold weather.

#### CAUSE:

------

The stabilizer shaft link insulator material may compress over a period of time. New parts with a different insulator material have been used in production since June, 1993.

#### CORRECTION:

-----------

Replace the stabilizer shaft link assemblies with new P/N 25621457. Refer to Section 3C in the Service Manual.

Labor Operation; E2147

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.