For 1990-2009 cars

# INTERMEDIATE STEERING SHAFT BOLT LOOSE

#### MODELS/YEARS 1990 NINETY-EIGHT

#### CONDITION

Some 1990 Ninety-Eight vehicles may have a steering shaft bolt that has not been tightened to specified torque. This condition causes a rattle which could be annoying, but cannot cause steering shaft separation. The vehicies affected are included within the following VIN mnge:

L4301942 - L4302633

Most of these vehicles do not have this condition. A list of the VINS of vehicles with this condition will be sent to dealers to whom those vehicles were shipped. To repair this condition, the intermediate steering shaft upper bolt should be tightened to 47 N. m (35 lbs.ft.) using the following procedure:

1. Remove left-hand instrument panel sound insulator panel (hush panel).

2. Pull top podion of dust cover down.

3. Torque pinch bolt to 47 N.m (35 lbs.ft.)

4. Pull dust cover up and secure back into position.

5. Reinstall sound insulator panel.

#### IMPORTANT: Refer to the 1990 Eighty-Eight and Ninety-Eight Service Manual, page 3F2-4, Figure 6 or Page 3F4-4, Figure 6.

#### WARRANTY INFORMATION

Labor Operation Number: T6391 Labor Time: .2 Hours. Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.