Restricted Exhaust System Check. Oldsmobile Shelby Series 1 1999

For 1990-2009 cars

#### Restricted Exhaust System Check

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain On-Board Diagnostic (OBD) System Check? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check

2

1. Remove the front heated oxygen sensor (HO2S) on the side of the engine that is suspected of being restricted. Refer to Heated Oxygen Sensor Replacement - Bank 2 Sensor 1 or Heated Oxygen Sensor Replacement - Bank 2 Sensor 2 .
2. Install the J 35314-A exhaust back pressure tester in place of the HO2S.
3. Idle the engine at normal operating temperature.
4. Observe the exhaust system back pressure reading on the gauge.

Does the reading exceed the specified value?

8.6 kPa (1.25 psi)

Go to Step 4

Go to Step 3

3

1. The J 35314-A exhaust back pressure gauge is still installed.
2. Increase engine speed to 2,000 RPM.
3. Observe the exhaust system back pressure reading on the gauge.

Does the reading exceed the specified value?

20.7 kPa (3 psi)

Go to Step 4

Go to Symptoms

4

1. Turn OFF the engine.
2. Reinstall the front HO2S.
3. Remove the rear HO2S on the side of the engine that is suspected of being restricted. Refer to Heated Oxygen Sensor Replacement - Bank 2 Sensor 1 or Heated Oxygen Sensor Replacement - Bank 2 Sensor 2 .
4. Install the J 35314-A exhaust back pressure tester in place of the HO2S.
5. Idle the engine.
6. Increase the engine speed to 2,000 RPM.
7. Observe the exhaust system back pressure reading on the gauge.

Does the reading exceed the specified value?

20.7 kPa (3 psi)

Go to Step 5

Go to Step 6

5

Repair the restriction in the exhaust system after the catalytic converter. Inspect the exhaust system for the following:

• | Collapsed pipe

• | Heat distress

• | Internal muffler failure

Is the action completed?

--

System OK

--

6 | Replace the catalytic converter. Is the action completed? | -- | System OK | --