DTC P0462 Fuel Level Sensor Circuit Low Voltage. Oldsmobile Shelby Series 1 1999

For 1990-2009 cars
Engine Controls Components
Fuel System
OBD II Symbol Description Notice
Powertrain Control Module Connector End Views
Handling ESD Sensitive Parts Notice

### Circuit Description

The fuel level sensor changes resistance based on fuel level. The fuel level sensor has a signal circuit and a ground circuit. Thepowertrain control module (PCM) applies about 5.0 volts on the signal circuit to the sensor. The PCM monitors changes in this voltage caused by changes in the resistance of the sensor to determine fuel level.

When the fuel tank is full, the sensor resistance is high, and the PCM signal voltage is only pulled down a small amount through the sensor to ground. Therefore, the PCM will sense a high signal voltage or full fuel tank. When the fuel tank is empty, the sensor resistance is low, and the signal voltage is pulled down a greater amount. This causes the PCM to sense a low signal voltage or empty fuel tank empty.

The PCM uses inputs from the fuel level sensor in order to calculate the total fuel remaining in the fuel tank. The PCM uses the fuel level information for the evaporative emission (EVAP) and misfire diagnostics. The fuel level information is sent to the instrument panel cluster (IPC) via the PCM. The instrument panel (IP) controls the fuel gauge based on the PCM signal.

This diagnostic trouble code (DTC) sets when the PCM senses a signal voltage lower than the normal operating range of the sensor.

### Conditions for Running the DTC

The engine is operating.

### Conditions for Setting the DTC

• | The fuel level sensor voltage is below 0.39 volts.

• | All conditions are present for 3.0 minutes.

### Action Taken When the DTC Sets

• | The PCM stores the DTC information into memory when the diagnostic runs and fails.

• | The malfunction indicator lamp (MIL) will not illuminate.

• | The PCM records the operating conditions at the time the diagnostic fails. The PCM stores this information in the Failure Records.

• | The fuel gauge displays empty.

### Conditions for Clearing the DTC

• | A History DTC will clear after 40 consecutive warm-up cycles, if no failures are reported by this or any other non-emission related diagnostic.

• | A last test failed, current DTC, will clear when the diagnostic runs and does not fail.

• | Use a scan tool in order to clear the DTC.

### Diagnostic Aids

Important: Remove any debris from the PCM connector surfaces before servicing the PCM. Inspect the PCM connector gaskets when diagnosing or replacing the PCM. Ensure that the gaskets are installed correctly. The gaskets prevent water intrusion into the PCM.

Depending on the current fuel level, it may be difficult to locate a malfunctioning sending unit. The malfunction may only occur when the fuel level is full or near empty. The fuel sending unit may need to be removed for further diagnosis. A fuel level sensor that has an intermittent condition causes this DTC to set. Remove the fuel sender assembly. Refer to Fuel Sender Assembly Replacement in order to test the resistance of the sensor. The resistance of the sensor should change smoothly. Replace the sensor if the resistance did not change smoothly.

With this DTC set, the vehicle fuel gauge displays empty.

The PCM will not reset the mileage for this diagnostic if the fuel tank is refueled to the same level as before the repair was made. Perform the following procedure in order to refuel the vehicle after replacing a sending unit or fuel tank:

1. Add 25 percent of the fuel that you removed before the repair.
2. Start and idle the engine for 5 minutes.
3. Turn OFF the engine.
4. Add the remainder of the fuel.

For an intermittent, refer to Symptoms .

### Test Description

The number below refers to the step number on the diagnostic table.

1. This step determines if the fault is present.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain On-Board Diagnostic (OBD) System Check ? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check

2

1. Install the scan tool.
2. Turn ON the ignition leaving the engine OFF.
3. Monitor the fuel level sensor display on the scan tool.

Is the fuel level sensor below the specified value?

0.39 V

Go to Step 4

Go to Step 3

3

1. Turn ON the ignition leaving the engine OFF.
2. Review the Freeze Frame and/or Failure Records data for this DTC and observe the parameters.
3. Turn OFF the ignition for 15 seconds.
4. Start the engine.
5. Operate the vehicle within the conditions required for this diagnostic to run, and as close to the conditions recorded in Freeze Frame and/or Failure Records as possible. Special operating conditions that you need to meet before the PCM will run this diagnostic, where applicable, are listed in Conditions for Running the DTC.
6. Select the Diagnostic Trouble Code (DTC) option and the Specific DTC option, then enter the DTC number using the scan tool.

Does the scan tool indicate that this diagnostic failed this ignition?

--

Go to Step 4

Go to Diagnostic Aids

4

1. Turn OFF the ignition.
2. Disconnect the fuel sender assembly electrical connector.
3. Turn ON the ignition leaving the engine OFF.
4. Observe the fuel level sensor display on the scan tool.

Is the fuel level sensor voltage below the specified value?

0.39 V

Go to Step 5

Go to Step 7

5

1. Turn OFF the ignition.
2. Disconnect the PCM connector C2 located on the opposite side of the manufacturers logo. Refer to Powertrain Control Module Replacement/Programming .
3. Test the fuel level sensor signal circuit for a grounded circuit. Refer to Testing for Short to Ground in Wiring Systems.

Is the fuel level sensor signal circuit grounded ?

--

Go to Step 6

Go to Step 8

6 | Repair the grounded fuel level signal circuit between the PCM connector and the fuel sender assembly. Refer to Wiring Repairs in Wiring Systems. Is the action complete? | -- | Go to Step 9 | --
7 | Replace the fuel sender assembly. Refer to Fuel Sender Assembly Replacement . Is the action complete? | -- | Go to Step 9 | --
8 | Important:: The replacement PCM must be programmed. Replace the PCM. Refer to Powertrain Control Module Replacement/Programming . Is the action complete? | -- | Go to Step 9 | --

9

1. Select the Diagnostic Trouble Code (DTC) option and the Clear DTC Information option using the scan tool.
2. Idle the engine at the normal operating temperature.
3. Select the Diagnostic Trouble Code (DTC) option and the Specific DTC option, then enter the DTC number using the scan tool.
4. Operate the vehicle within the Conditions for Running the DTC as specified in the supporting text, if applicable.

Does the scan tool indicate that this test ran and passed?

--

Go to Step 10

Go to Step 2

10 | Select the Capture Info option and the Review Info option using the scan tool. Does the scan tool display any DTCs that you have not diagnosed? | -- | Go to the applicable DTC table | System OK