PARKING LAMP TO FASCIA GAPPING (INSTALL NEW SHIM). Oldsmobile Toronado 1990

For 1990-2009 cars

# PARKING LAMP TO FASCIA GAPPING (INSTALL NEW SHIM)

#### MODELS/YEARS 1990 TORONADO AND TROFEO

Some 1990 Toronados or Trofeos may experience a gapping condition between the parking lamp and the bumper fascia. To correct this condition, fabricate shim using pattern provided (refer to Figure 1) out of 1/16" shim stock and install between the energy absorber unit and the bumper reinforcement as shown in Figure 2.

#### NOTE: More than one shim may be required depending on size of gap.

#### WARRANTY INFORMATION:

Labor Operation Number: B0260 Labor Time: 0.4 hours Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.