QUARTER TRIMLOOSE FIT ALONG BACKLITE & SAIL AREA. Oldsmobile Toronado 1990

For 1990-2009 cars

# QUARTER TRIMLOOSE FIT ALONG BACKLITE & SAIL AREA

#### SUBJECT QUARTER TRIM LOOSE ALONG BACK GLASS AND SAIL AREA (REPLACE QUARTER TRIM RETAINERS)

#### MODELS/YEARS 1990 TORONADO AND TROFEO MODELS

Some 1990 Toronado and Trofeo models may exhibit a condition where the quarter trim may be loose along the back glass and sail area. This may be caused by insufficient retention of the quarter trim retainers (Christmas tree fasteners) to the sheet metal. To repair this condition use the following procedure:

1. Remove coat hook.

2. Remove assist strap covers and assist strap screws.

3. Pull quarter trim away from sheet metal to access quarter trim retainers.

4. Remove three quarter trim retainers. Refer to the illustration on the back of this bulletin.

5. Replace with P/N 20750175.

6. Push in quarter trim and replace coat hook and assist strap.

Parts are currently available from GMSPO.

#### WARRANTY INFORMATION:

Right Side - Labor Operation Number: T6502 Labor Time: 0.2 hour Trouble Code: 92

Left Side - Labor Operation Number: T6501 Labor Time: 0.2 hour Trouble Code: 92

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.