RIGHT COOLING FAN STALL REPL. FAN/ADD UNDERBODY SCREEN. Oldsmobile Toronado 1992

For 1990-2009 cars

# RIGHT COOLING FAN STALL REPL. FAN/ADD UNDERBODY SCREEN

#### SUBJECT: RIGHT COOLING FAN STALL (REPLACE COOLING FAN AND ADD AN UNDERBODY SCREEN)

#### VEHICLES AFFECTED: 1990-92 OLDSMOBILE TORONADO

Some 1990-1992 Oldsmobile Toronados prior to VIN breakpoint NU304238 may experience a stalling condition of the right cooling fan. This may be due to an ingestion of road debris by the fan motor. The aerodynamics of this vehicle allows ram air to be picked up from the road, which may be littered with plastic bags and wrappers. To prevent this condition, replace the damaged cooling fan, if necessary, and add an underbody screen which has been developed to protect the fan from ingesting road debris.

Part Description P/N ---------------- Right Cooling Fan Motor 22088877 Underbody Screen 3532321

To install the underbody screen (refer to the attached illustrations).

1. Raise vehicle

2. Remove five (10mm) screws securing air deflector

3. Insert screen into upper fascia

4. Install rear of screen above air deflector and align screen and deflector attachment holes

5. Return five (10mm) screws to secure screen and deflector

6. Lower vehicle

For vehicles repaired under warranty use:

Right-Hand Cooling Fan J3400 .4 Underbody Screen .3

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.