CONSOLE COIN/CUP HOLDER BINDS (DIAGNOSTIC PROCEDURE). Oldsmobile Toronado 1987

For 1990-2009 cars

# CONSOLE COIN/CUP HOLDER BINDS (DIAGNOSTIC PROCEDURE)

#### MODELS/YEARS: 1986-89 TORONADO

Some 1986-1989 Toronado vehicles equipped with a center console may experience a condition where the coin/cup holder binds or requires excessive effort to operate. This condition may be caused by any of the following:

- Interference of the coin/cup holder with console wiring.

- Distorted coin/cup mounting plate.

- Defective coin/cup mounting plate.

To repair this condition use the following procedure:

1. Remove console trim plate.

2. Remove shift indicator assembly.

3. Remove coin/cup mounting plate assembly.

4. Refer to trouble tree. (Figure 1)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.