PARKING LAMP TO FASCIA GAPPING (INSTALL NEW SHIM). Oldsmobile Toronado 1990

For 1990-2009 cars

# PARKING LAMP TO FASCIA GAPPING (INSTALL NEW SHIM)

#### VEHICLES AFFECTED: 1990 'E'

Some 1990 Oldsmobile Toronados or Trofeos may experience a gapping condition between the parking lamp and the bumper fascia. To correct this condition, fabricate shim using pattern provided (refer to Figure 2) out of 1/16" shim stock and install between the energy absorber unit and the bumper reinforcement as shown in Figure 1.

#### NOTE: More than one shim may be required depending on size of gap.

Use most applicable labour operation and time from the Canadian Labour Time Guide.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.