REVISED REAR ALIGNMENT SPECIFICATIONS. Oldsmobile Toronado 1983

For 1990-2009 cars

# REVISED REAR ALIGNMENT SPECIFICATIONS

#### VEHICLES AFFECTED: 1979-1984 Eldorado 1980-1984 Seville

Some 1979-1984 Eldorados and 1980-1984 Sevilles may experience irregular rear tire wear. If this condition is encountered, the following corrective action should be taken:

Check rear wheel aligment. Reset toe-in (if necessary) to the following specifications.

Per Wheel: 0.10 DEG + 0.10 DEG (0.05' + 0.05') Sum: 0.20 DEG + 0.20 DEG (0.10' + 0.10')

If tires are not excessively worn, rotate tires in a 'Modified X' pattern as shown in Figure 1.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.