IRREGULAR/PREMATURE TIRE WEAR REPAIR/ROTATION PROCEDURE. Oldsmobile Toronado 1986

For 1990-2009 cars

# IRREGULAR/PREMATURE TIRE WEAR REPAIR/ROTATION PROCEDURE

IRREGULAR/PREMATURE TIRE WEAR - ALL-SEASON TIRES

1985 TORONADO & 1985-86 CUTLASS CIERA REAR POSITION ONLY 1985 DELTA 88 & 1985-86 CUTLASS SUPREME FRONT POSITION ONLY

This information is a supplement to Dealer Technical Bulletin 86-T-35 issued May 14, 1986.

Under Service Procedure, please note for dealers in the state of Ohio the telephone number for General Tire is 1-800-426-4889.

Also please add the following to Warranty information:

Labor Operation Labor Model Description Number Hours ----- ----------- --------- ----- Cutlass Supreme Rotate Tires & Align T-5108 1.4 Front Suspension

Cutlass Supreme Replace Front Tires & Firestone Tires T-5109 2.0 Align Front Suspension General Tires T-5110 Goodyear Tires T-5111 Uniroyal Tires T-5112

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.