For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A-Pillar Fender Bolt | 10 N·m | 89 lb in
Door Hinge to Body Bolts | 2.5 N·m | 22 lb in
Door Hold Open Link to Body Bolts | 10 N·m | 89 lb in
Front Fascia-to-Fender Bolts | 20 N·m | 15 lb ft
Front of Fender Bolts | 20 N·m | 15 lb ft
Fuel Filler Door Screws | 12 N·m | 106 lb in
Hinge Bolts | 2 N·m | 18 lb in
Hood Latch Bolts | 10 N·m | 89 lb in
Hood-to-Hinge Bolts | 4.5 N·m | 40 lb in
Hood Release Handle Screw | 10 N·m | 89 lb in
Lift Gate Hinge Bolts | 27.5 N·m | 20 lb ft
Lift Gate Latch Bolts | 20 N·m | 15 lb ft
Lower Fender Bolts | 4 N·m | 35 lb in
Radiator Grille Nuts | 25 N·m | 18 lb in
Upper Fender Bolts | 10 N·m | 89 lb in