For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat from the vehicle. Refer to Rear Seat Replacement .
2. Remove the screws and the rear seat trim.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear seat trim with the screws.

Tighten
Tighten the rear seat trim screws to 12 N·m (9 lb ft).

2. Install the rear seat from the vehicle. Refer to Rear Seat Replacement .