For 1990-2009 cars

## Hood Ajar Indicator Switch Replacement C100/Long Body

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the hood safety switch.
3. Disconnect the electrical connector from the hood safety switch.

### Installation Procedure

1. Connect the electrical connector to the hood safety switch.
2. Install the hood safety switch.
3. Connect the negative battery cable.

## Hood Ajar Indicator Switch Replacement C105/Short Body

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the bolts and the hood latch.
3. Disconnect the electrical connector from the hood safety switch.
4. Remove the hood safety switch from the hood latch.

### Installation Procedure

1. Install the hood safety switch to the hood latch.
2. Connect the electrical connector to the hood safety switch.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the hood latch and bolts.

Tighten
Tighten the hood latch bolts to 10 N·m (7 lb ft).

4. Connect the negative battery cable.