For 1990-2009 cars

## Quarter Lower Rear Trim Panel Replacement C 100/Long Body

### Removal Procedure

1. Remove the rear seat lower bolts. Refer to Seat Belt Retractor Replacement - No. 1 Rear and Seat Belt Retractor Replacement - No. 2 Rear .
2. Remove the rear compartment stow tray. Refer to Rear Storage Compartment Replacement .
3. Remove the screws and the rear quarter lower trim panel.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear quarter lower trim panel with the screws.

Tighten
Tighten the rear trim panel screws to 2 N·m (18 lb in).

2. Install the rear compartment stow tray. Refer to Rear Storage Compartment Replacement .
3. Install the rear seat lower bolts. Refer to Seat Belt Retractor Replacement - No. 1 Rear and Seat Belt Retractor Replacement - No. 2 Rear .

## Quarter Lower Rear Trim Panel Replacement C 105/Short Body

### Removal Procedure

1. Remove the rear seat lower bolts. Refer to Seat Belt Retractor Replacement - No. 1 Rear and Seat Belt Retractor Replacement - No. 2 Rear .
2. Remove the rear compartment stow tray. Refer to Rear Storage Compartment Replacement .
3. Remove the screws and the rear quarter lower trim panel.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the rear quarter lower trim panel with the screws.

Tighten
Tighten the rear trim panel screws to 2 N·m (18 lb in).

2. Install the rear compartment stow tray. Refer to Rear Storage Compartment Replacement .
3. Install the rear seat lower bolts. Refer to Seat Belt Retractor Replacement - No. 1 Rear and Seat Belt Retractor Replacement - No. 2 Rear .