For 1990-2009 cars

### Disassembly Procedure

1. Remove the clutch master cylinder assembly from the vehicle. Refer to Clutch Master Cylinder Replacement .
2. Remove the boot and disconnect the piston stop ring using ring pliers.
3. Remove the pushrod assembly and the piston assembly.

### Assembly Procedure

1. Apply clean fluid to the piston assembly cup and insert the piston assembly and the pushrod assembly into the master cylinder body.
2. Install the piston stop ring using ring pliers. Install the boot.
3. Install the clutch master cylinder assembly into the vehicle. Refer to Clutch Master Cylinder Replacement .