For 1990-2009 cars

### Removal Procedure

1. Remove the transmission control valve body cover. Refer to Control Valve Body Cover Replacement.
2. Disconnect the input speed sensor electrical connector (1).
3. Remove the input speed sensor bolt (2) M6 x 23.
4. Remove the input speed sensor (3).
5. Remove the 3 input speed sensor seals (1).

### Installation Procedure

1. Install the 3 input speed sensor seals (1).
2. Install the input speed sensor (3).

Caution: Refer to Fastener Caution in the Preface section.

3. Install the input speed sensor bolt (2) M6 x 23 and tighten to 12 N·m (106 lb in).
4. Connect the input speed sensor electrical connector (1).
5. Install the transmission control valve body cover. Refer to Control Valve Body Cover Replacement.

Perform the service fast learn adapt procedure. Refer to Service Fast Learn Adapts.