For 1990-2009 cars

## Front Door Frame Applique Replacement C100/Long Body

### Removal Procedure

1. Reposition the weatherstrip in order to access the screws.
2. Remove the screws and the front side door window frame applique.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the screws and the Front side door window frame applique.

Tighten
Tighten the front side door window frame applique screws to 1.3 N·m (12 lb in).

2. Install the weatherstrip to its original position.

## Front Door Frame Applique Replacement C105/Short Body

### Removal Procedure

1. Remove the front door applique screws.
2. Remove the front door frame applique.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the front door frame applique.
2. Install the screws to the front door frame applique.

Tighten
Tighten the front door applique screws to 1.3 N·m (12 lb in).