For 1990-2009 cars

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
3. Visually check the brake pads for minimum thickness and wear.
4. Measure the thickness. Refer to Disc Brake Component Specifications.
5. Install the brake shoes in axle sets only.
6. Install the tire and wheel assembly. Refer to Tire and Wheel Removal and Installation.
7. Lower the vehicle.