For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Automatic Transaxle to Engine Bolt | 75 N·m | 55 lb ft
Control Valve Body Bolt | 10 N·m | 89 lb in
Control Valve Body Cover Bolt | 13 N·m | 115 lb in
Drain Plug | 40 N·m | 30 lb ft
Engine to Transaxle Brace Bolt | 50 N·m | 37 lb ft
Fluid Level Indicator Bolt | 10 N·m | 89 lb in
Frame to Body Bolt | 155 N·m | 114 lb ft
Fuel Hose/Pipe Retainer Nut | 28 N·m | 21 lb ft
Input Speed Sensor Bolt | 6 N·m | 53 lb in
Left Transaxle Mount to Side Rail Bolt | 37 N·m | 27 lb ft
Left Transaxle Mount to Transaxle Bolt | 50 N·m | 37 lb ft
Negative Battery Cable to Transaxle Nut | 45 N·m | 33 lb ft
Output Speed Sensor Bolt | 6 N·m | 53 lb in
Rear Transaxle Mount Bracket Bolt | 55 N·m | 41 lb ft
Rear Transaxle Mount to Rear Transaxle Mount Bracket Bolt | 110 N·m | 80 lb ft
Shift Control Assembly Nut | 25 N·m | 18 lb ft
Shift Control Cable Bracket Bolt | 25 N·m | 18 lb ft
Shift Control Knob Screw | 1.5 N·m | 13 lb in
Steering Gear to Frame Bolts | 110 N·m | 81 lb ft
Steering Intermediate Shaft Pinch Bolt | 34 N·m | 25 lb ft
Torque Converter Bolt | 60 N·m | 44 lb ft
Transaxle Manual Shaft Nut | 7 N·m | 62 lb in
Transaxle Range Switch Bolt | 25 N·m | 18 lb ft
Transaxle Range Switch Lever Nut | 16 N·m | 12 lb ft
Transaxle Range Switch Stud | 25 N·m | 18 lb ft
Transaxle Case to Transaxle Bolt | 60 N·m | 44 lb ft
Transaxle Oil Cooler Line Fitting | 16 N·m | 12 lb ft
Transaxle Oil Cooler Line Retaining Nut | 7 N·m | 62 lb in
Transfer Case to Transaxle Bolts | 60 N·m | 44 lb ft
Transmission Test Hole Plug | 7 N·m | 62 lb in