For 1990-2009 cars

## Quarter Window Replacement Long Body C/100

### Removal Procedure

1. Remove the quarter window garnish molding. Refer to Body Side Window Rear Garnish Molding Replacement .
2. Remove the nuts and the outer window.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the outer window with the nuts.

Tighten
Tighten the outer window nuts to 6 N·m (53 lb in).

2. Install the quarter window garnish molding. Refer to Body Side Window Rear Garnish Molding Replacement .

## Quarter Window Replacement Short Body C/105

### Removal Procedure

1. Disconnect the negative battery cable, if equipped with glass breakage detector. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the quarter window garnish molding. Refer to Body Side Window Rear Garnish Molding Replacement .
3. Disconnect the glass breakage detector connector (1), if equipped.
4. Remove the nuts and the outer window.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the outer window with the nuts.

Tighten
Tighten the outer window nuts to 6 N·m (53 lb in).

2. Connect the glass breakage detector connector (1), if equipped.
3. Install the quarter window garnish molding. Refer to Body Side Window Rear Garnish Molding Replacement .
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.