For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the front wheel. Refer to Tire and Wheel Removal and Installation.
3. Remove the front mud guard. Refer to Rear Mud Flap Guard Replacement.
4. Remove the engine protection shield. Refer to Engine Protection Shield Replacement.
5. Remove the screws and the front fender liner.

### Installation Procedure

Caution: Refer to Title not found in the Preface section.

1. Install the screws and the front fender liner and tighten to 4 N·m (35 lb in).
2. Install the engine protection shield. Refer to Engine Protection Shield Replacement.
3. Install the front mud guard. Refer to Rear Mud Flap Guard Replacement.
4. Install the front wheel. Refer to Tire and Wheel Removal and Installation.
5. Lower the vehicle.