For 1990-2009 cars

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the headliner. Refer to Headlining Trim Panel Replacement .
3. Remove the drain hoses.
4. Disconnect the electrical connectors.
5. Remove the screws and the motor.
6. Remove the motor control module.
7. Remove the bolts and the housing from the vehicle.
8. Remove the rubber end caps.
9. Remove the drain nozzles.
10. Remove the shade stops.
11. Remove the glass stops.
12. Remove the shade.
13. Remove the glass and the frame from the housing.
14. Remove the plastic trim.
15. Remove the screws and the glass from the frame.

### Installation Procedure

1. Install the glass to the frame with the screws.
2. Install the plastic trim.
3. Install the glass and the frame to the housing.
4. Install the shade.
5. Install the glass stops.
6. Install the shade stops.
7. Install the drain nozzles.
8. Install the rubber end caps.

Notice: Refer to Fastener Notice in the Preface section.

9. Install the housing to the roof of the vehicle with the bolts.

Tighten
Tighten the sunroof housing bolts to 10 N·m (89 lb in).

10. Install the motor control module.
11. Install the motor with the screws.

Tighten
Tighten the sunroof motor screws to 3 N·m (27 lb in).

12. Connect the electrical connectors.
13. Install the drain hoses.
14. Install the headliner. Refer to Headlining Trim Panel Replacement .
15. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .