For 1990-2009 cars

#### Tools Required

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

1. Remove the battery and battery tray. Refer to Battery Tray Replacement .
2. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement .

Important: Only lift the engine far enough to take the weight off the transaxle front mount assembly, or damage to the mount and lifting equipment failure may occur.

3. Support the engine assembly using the DW-110-060 .
4. Remove the transaxle mount bracket retaining bolts from the transaxle.
5. Remove the transaxle mount assembly retaining bolts from the left front longitudinal.
6. Remove the transaxle mount assembly.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the transaxle mount assembly.

Tighten

• | Tighten the transaxle mount assembly retaining bolts (2) to 37 N·m (27 lb ft).

• | Tighten the transaxle mount bracket retaining bolts (1) to 50 N·m (37 lb ft).

2. Remove DW-110-060 .
3. Install the battery and battery tray. Refer to Battery Tray Replacement .
4. Install the engine dress cover. Refer to Fuel Injector Sight Shield Replacement .