For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedure

It is only necessary to lower the headliner. Only perform the steps in the headliner replacement procedure that will lower the headliner enough to gain access to the part. Refer to Headlining Trim Panel Replacement .

1 | Sunroof Motor/Actuator Screws (Qty: 3) Notice: Refer to Fastener Notice in the Preface section.

#### Procedure

1. The sunroof window must be in the fully closed position before disconnecting the harness, to ensure synchronization of the sunroof motor to the sunroof module.
2. Disconnect the electrical connector from the sunroof motor.

Tighten
Tighten the screws to 5 N·m (44 lb in).

2 | Sunroof Motor/Actuator

#### Procedure

1. Pull downward to disengage the motor/actuator from the sunroof module.
2. Install the motor, verify the sunroof operation.
3. Ensure the motor/actuator initialization/teach process has been done. Refer to Sunroof Motor/Actuator Initialization/Teach Process .
4. Install the headliner. Refer to Headlining Trim Panel Replacement .