For 1990-2009 cars

### Removal Procedure

1. Remove the rear brake rotor. Refer to Rear Brake Rotor Replacement.
2. Remove the upper return spring, lower return spring and adjuster assembly from the park brake shoe.
3. Remove the retaining spring plate, spring and retaining spring pin.
4. Remove the park brake shoe.

### Installation Procedure

1. Install the retaining spring pin, park brake shoe, retaining spring and retaining spring plate.
2. Install the adjuster assembly, lower return spring and upper return spring.
3. Install the rear brake rotor. Refer to Rear Brake Rotor Replacement.