For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

Important: Only lift the engine far enough to take the weight off the transaxle front mount assembly, or damage to the mount and lifting equipment failure may occur.

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.
2. Support the engine assembly using DW-110-060 .
3. Remove the transfer case. Refer to Transfer Case Assembly Replacement.
4. Remove the transaxle rear mount-to-bracket through bolt.
5. Remove the transaxle rear mount bracket retaining bolts and nuts from the transaxle.
6. Remove the transaxle rear mount bracket.
7. Remove the transaxle rear mount retaining bolts from the cradle.
8. Remove the transaxle rear mount.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the transaxle rear mount to the cradle.

Tighten
Tighten the transaxle rear mount retaining bolts to 90 N·m (66 lb ft).

2. Install the transaxle rear mount bracket to the transaxle.

Tighten
Tighten the transaxle rear mount bracket retaining bolts to 90 N·m (66 lb ft).

Important: Before tightening the transaxle rear mount through bolt, swing the engine assembly backwards and forwards or from the side to side for the proper alignment.

3. Install the transaxle rear mount through bolt.

Tighten
Tighten the transaxle rear mount-to-bracket through bolt to 90 N·m (66 lb ft).

4. Install the transfer case. Refer to Transfer Case Assembly Replacement.
5. Remove DW-110-060 .
6. Install the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement.