For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the lamp. Refer to Headlamp Replacement.
3. Twist and remove the bulbs from the headlamp.

### Installation Procedure

1. Insert and twist to install the replacement bulb into the headlamp.
2. Connect the electrical connector.
3. Install the headlamp. Refer to Headlamp Replacement.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.