For 1990-2009 cars

### Removal Procedure

Note: Left-Hand Drive Shown, Right-Hand Drive Similar.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the screws at the base of the storage compartment.
3. Open and remove the screws.
4. Disconnect the electrical connector.
5. Remove the storage compartment.

### Installation Procedure

1. Position the storage compartment in the instrument panel.
2. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the storage compartment with the screws and tighten to 2 N·m (18 lb in).
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.