For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear wheel. Refer to Tire and Wheel Removal and Installation .
3. Disconnect the electrical connector (1) from the rear wheel speed sensor.
4. Remove the bolt (2) and the rear wheel speed sensor (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the bolt (2) and rear wheel speed sensor (1).

Tighten
Tighten the bolt to 8 N·m (71 lb in).

2. Connect the electrical connector (1) to the rear wheel speed sensor.
3. Install the rear wheel. Refer to Tire and Wheel Removal and Installation .
4. Lower the vehicle.