For 1990-2009 cars

### Removal Procedure

Note: Left-Hand Drive Shown, Right-Hand Drive Similar.

1. Remove the hood prime latch release handle. Refer to Hood Primary Latch Release Cable Replacement.
2. Remove the screw and the instrument panel lower left trim.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the instrument panel lower left trim and tighten the instrument panel steering column opening pillar screw to 2 N·m (18 lb in).
2. Install the hood prime latch release handle. Refer to Hood Primary Latch Release Cable Replacement.