For 1990-2009 cars

## Headlamp Leveling Switch Replacement C100/Long Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument cluster steering column opening pillar.
3. Remove the screw and the headlamp leveling switch.
4. Disconnect the electrical connectors.

### Installation Procedure

1. Replace the appropriate switch.
2. Connect the electrical connectors.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the headlamp leveling switch with the screw and tighten to 2 N·m (18 lb in).
4. Install the instrument cluster steering column opening pillar.
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

## Headlamp Leveling Switch Replacement C105/Short Body

### Removal Procedure

Note: Left - Hand Drive Shown, Right - Hand Drive Similar.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the instrument cluster steering column opening pillar.
3. Remove the screw and the headlamp leveling switch.
4. Disconnect the electrical connectors.

### Installation Procedure

1. Replace the appropriate switch.
2. Connect the electrical connectors.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the headlamp leveling switch with the screw and tighten to 2 N·m (18 lb in).
4. Install the instrument cluster steering column opening pillar.
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.