For 1990-2009 cars

#### Special Tools

• | J-45201 Cooler Line Seal Remover

• | J-46626 Seal Installer

### Removal Procedure

1. Remove the battery tray. Refer to Battery Tray Replacement.
2. Remove the manual shaft and position switch assembly. Refer to Manual Shift Detent Lever with Shaft Position Switch Assembly Replacement.
3. Remove the manual shaft seal using J 45201 .

### Installation Procedure

1. Install the manual shaft and position switch assembly. Refer to Manual Shift Detent Lever with Shaft Position Switch Assembly Replacement.
2. Install the manual shaft seal using J-46626 .
3. Install the battery tray. Refer to Battery Tray Replacement.