For 1990-2009 cars

### Removal Procedure

1. Set the park brake and chock the wheels.
2. Disconnect the transmission range selector lever cable terminal (1) from the transmission manual shift lever pin.
3. Press the locking tabs inward in order to release the transmission range selector lever cable (2) from the cable bracket.
4. Remove the transmission range selector lever nut (1).
5. Remove the transmission range selector lever (2).

### Installation Procedure

1. Install the transmission range selector lever (2).

Caution: Refer to Fastener Caution in the Preface section.

2. Install the transmission range selector lever nut (1) and tighten to 20 N·m (15 lb ft) .
3. Install the transmission range selector lever cable (2) to the cable bracket.
4. Connect the transmission range selector lever cable terminal (1) to the transmission manual shift lever pin.
5. Check the range selector cable adjustment. Refer to Range Selector Lever Cable Adjustment .