For 1990-2009 cars

Connector 1: | Fuseblock - I/P X1
Connector 2: | Fuseblock - I/P X2
Connector 3: | Fuseblock - Underhood X1
Connector 4: | Fuseblock - Underhood X3
Connector 5: | Ignition Switch

### Fuseblock - I/P X1

#### Connector Part Information

- OEM: TYCO 0-1743134-2
- Service: N/A
- Description: 60-Way F Unsealed

#### Fuseblock X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | -- | -- | Not Used
2 | YE | -- | Accessory Voltage
3-9 | -- | -- | Not Used
10 | PK | -- | Run/Crank Ignition 1 Voltage
11 | PK | -- | Run/Crank Ignition 1 Voltage
12 | PK | -- | Run/Crank Ignition 1 Voltage
13 | -- | -- | Not Used
14 | RD/WH | -- | Battery Positive Voltage
15-16 | -- | -- | Not Used
17 | YE | -- | Accessory Voltage
18 | YE | -- | Accessory Voltage
19 | PK | -- | Run/Crank Ignition 1 Voltage
20-21 | -- | -- | Not Used
22 | RD/WH | -- | Battery Positive Voltage
23-24 | -- | -- | Not Used
25 | PK | -- | Run/Crank Ignition 1 Voltage
26 | YE | -- | Run/Crank Ignition 1 Voltage
27-28 | -- | -- | Not Used
29 | RD/WH | -- | Battery Positive Voltage
30 | RD/WH | -- | Battery Positive Voltage
31 | -- | -- | Not Used
32 | PK | -- | Run/Crank Ignition 1 Voltage
33-34 | -- | -- | Not Used
35 | RD/WH | -- | Battery Positive Voltage
36-37 | -- | -- | Not Used
38 | RD/WH | -- | Battery Positive Voltage
39-40 | -- | -- | Not Used
41 | RD/WH | -- | Battery Positive Voltage
42 | RD/WH | -- | Battery Positive Voltage
43 | BN | -- | Run Ignition 3 Voltage
44-45 | -- | -- | Not Used
46 | RD/WH | -- | Battery Positive Voltage
47-48 | -- | -- | Not Used
49 | RD/WH | -- | Battery Positive Voltage
50 | RD/WH | -- | Battery Positive Voltage
51-53 | -- | -- | Not Used
54 | RD/WH | -- | Battery Positive Voltage
55-56 | -- | -- | Not Used
57 | RD/WH | -- | Battery Positive Voltage
58 | RD/WH | -- | Battery Positive Voltage
59 | BN | -- | Run Ignition 3 Voltage
60 | BN | -- | Run Ignition 3 Voltage

### Fuseblock - I/P X2

#### Connector Part Information

- OEM: TYCO 0-1743134-3
- Service: N/A
- Description: 60-Way F 110/250/375 Unsealed

#### Fuseblock To Block ASM - I/P Wiring Harness Junction X2

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | RD/WH | -- | Battery Positive Voltage
4 | OG | -- | Rear For Lamp Supply Voltage
5-6 | -- | -- | Not Used
7 | RD/WH | -- | Battery Positive Voltage
8 | BN | -- | Run Ignition 3 Voltage
9 | -- | -- | Not Used
10 | PK | -- | Run/Crank Ignition 1
11 | WH | -- | Rear Defog Relay Control
12 | PK | -- | Lift Glass/Trunk Exterior Release Signal
13 | RD/WH | -- | Battery Positive Voltage
14 | -- | -- | Not Used
15 | RD/WH | -- | Battery Positive Voltage
16 | BN | -- | Run Ignition 3 Voltage
17 | YE | -- | Accessory Voltage
18 | PK | -- | Run/Crank Ignition 1 Voltage
19 | PK | -- | Run/Crank Ignition 1 Voltage
20 | OG | -- | Windshield Washer Pump Control
21 | RD/WH | -- | Battery Positive Voltage
22-23 | -- | -- | Not Used
24 | BN | -- | Run Ignition 3 Voltage
25 | YE | -- | Run/Crank Relay Coil Control
26 | PK | -- | Run/Crank Ignition 1 Voltage
27 | BN | -- | Lift Glass/Trunk Motor Release Control
28 | RD/WH | -- | Battery Positive Voltage
29-30 | -- | -- | Not Used
31 | BN | -- | Rap Relay Coil Control
32 | PK | -- | Run/Crank Ignition 1 Voltage
33 | YE | -- | Rear Fog Lamp Relay Control
34 | RD/WH | -- | Battery Positive Voltage
35 | -- | -- | Not Used
36 | RD/WH | -- | Battery Positive Voltage
37 | YE | -- | Accessory Voltage
38 | YE | -- | Power Supply
49 | RD/WH | -- | Battery Positive Voltage
40-41 | -- | -- | Not Used
42 | RD/WH | -- | Battery Positive Voltage
43 | OG | -- | --
44 | BN | -- | Signal Ground
45 | YE | -- | Accessory Voltage
46 | -- | -- | Not Used
47 | GY | -- | Door Lock Actuator Lock Control
48 | RD/WH | -- | Battery Positive Voltage
49 | BN | -- | Door Lock Actuator Unlock Control
50 | -- | -- | Not Used
51 | RD/WH | -- | Battery Positive Voltage
52 | -- | -- | Not Used
53 | YE | -- | Accessory Voltage
54 | -- | -- | Not Used
55 | BN | -- | Driver Door Lock Actuator Unlock Control
56 | L-GN | -- | Left Front Door Lock Relay Control
57 | BK | -- | Ground
58 | PK/BK | -- | Engine Main Relay Fused Control (2)
59-60 | -- | -- | Not Used

### Fuseblock - Underhood X1

#### Connector Part Information

- OEM: TYCO 0-1743130-2
- Service: N/A
- Description: 55-Way Block Assembly Unsealed

#### Fuseblock X1

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | -- | Cooling Fan Motor Supply Volt (2)
2 | -- | -- | Not Used
3 | PK/BK | -- | Engine Main Relay Fused Control (2)
4 | PK/BK | -- | Engine Main Relay Fused Control (2)
5 | -- | -- | Not Used
6 | RD/WH | -- | Battery Positive Voltage
7 | PU | -- | Starter Solenoid Crank Voltage
8 | YE | -- | Starter Relay Coil Control
9-11 | -- | -- | Not Used
12 | PK/BK | -- | Engine Main Relay Fused Control (3)
13 | PK/BK | -- | Engine Main Relay Fused Control (3)
14 | PK/BK | -- | Engine Main Relay Fused Control (3)
15 | -- | -- | Not Used
16 | PK/BK | -- | Engine Main Relay Fused Control (4)
17 | PK/BK | -- | Engine Main Relay Fused Control (4)
18 | BN | -- | Engine Main Relay Fused Control
19 | -- | -- | Not Used
20 | PK/BK | -- | Engine Main Relay Fused Control (1)
21 | -- | -- | Not Used
22 | L-BU | -- | Cooling Fan Motor Supply Volt (1)
23-24 | -- | -- | Not Used
25 | D-GN | -- | A/C Comp Clutch Supply Volt
26 | PK/BK | -- | Engine Main Relay Fused Control (4)
27 | PK/BK | -- | Engine Main Relay Fused Control (4)
28 | BK | -- | Ground
29 | -- | -- | Not Used
30 | D-GN | -- | Low Speed Cooling Fan Relay Control
31-32 | -- | -- | Not Used
33 | WH | -- | Cooling Fan Motor Low Reference
34 | YE | -- | Trans PSN Switch B2 Signal
35 | -- | -- | Not Used
36 | RD/WH | -- | Battery Positive Voltage
37 | RD/WH | -- | Battery Positive Voltage
38 | -- | -- | Not Used
39 | BK/WH | -- | Signal Ground
40-42 | -- | -- | Not Used
43 | BN/WH | -- | Trans PSN Switch B1 Signal
44 | WH | -- | Trans PSN Switch PB Signal
45 | PK | -- | Run/Crank Ignition 1 Voltage
46 | D-GN/WH | -- | A/C Comp Clutch Relay Control
47 | -- | -- | Not Used
48 | D-GN/WH | -- | Fuel Pump Primary Relay Control
49-50 | -- | -- | Not Used
51 | GY | -- | Trans PSN Switch B3 Signal
52 | -- | -- | Not Used
53 | L-BU | -- | Stop Lamp Supply Voltage
54 | PK | -- | Run/Crank Ignition 1 Voltage
55 | L-GN | -- | High Speed Cooling Fan Relay Control
56 | -- | -- | Not Used

### Fuseblock - Underhood X3

#### Connector Part Information

- OEM: TYCO 1-1743130-3
- Service: N/A
- Description: 56-Way Block Assembly Unsealed

#### Fuseblock X3

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1-2 | -- | -- | Not Used
3 | D-BU/WH | -- | Right Front T/Signal Lamp Supply Voltage
4 | PU/WH | -- | Air Quality Sensor Signal
5 | BN | -- | Run Ignition 3 Voltage
6 | L-BU/WH | -- | Left Front T/Signal Lamp Supply Voltage
7 | BN/WH | -- | Windshield Washer Fluid Level Sensor Signal
8 | -- | -- | Not Used
9 | D-GN | -- | Rear Window Washer Pump
10-11 | -- | -- | Not Used
12 | PU | -- | Right Park Lamp Supply Voltage
13 | D-GN/WH | -- | Outside Ambient Air Temperature
14-15 | -- | -- | Not Used
16 | PU | -- | Hood Closed Switch Signal
17 | -- | -- | Not Used
18 | D-GN | -- | HDLP Leveling Motor Supply Voltage
19 | -- | -- | Not Used
20 | YE | -- | Left HDLP Low Beam Supply Voltage
21 | -- | -- | Not Used
22 | OG/BK | -- | Sensor Low Reference
23 | -- | -- | Not Used
24 | PU | -- | Front Fog Lamp Supply
25 | PU | -- | Front Fog Lamp Supply
26 | OG | -- | Windshield Washer Pump Control
27 | D-GN | -- | HDLP Leveling Motor Supply Voltage
28-29 | -- | -- | Not Used
30 | BN/WH | -- | Right HDLP Low Beam Supply Voltage
31-33 | -- | -- | Not Used
34 | D-GN/WH | -- | Left HDLP High Beam Supply Voltage
35-36 | -- | -- | Not Used
37 | BK | -- | Ground
38 | -- | -- | Not Used
39 | BN/WH | -- | Left Park Lamp Supply Voltage
40-42 | -- | -- | Not Used
43 | L-GN/BK | -- | Right HDLP High Beam Supply Voltage
44 | -- | -- | Not Used
45 | D-GN | -- | HDRN Control
46 | D-GN | -- | HDRN Control
47-53 | -- | -- | Not Used
54 | PU | -- | Headlamp Washer Pump Control
55-56 | -- | -- | Not Used

### Ignition Switch

#### Connector Part Information

- OEM: JAE IL-AG5-6S-S3C1
- Service: N/A
- Description: 6-Way F IL5 Unsealed

#### Ignition Switch

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE | -- | Accessory Voltage
2 | RD/WH | -- | Battery Positive Voltage
3 | PK | -- | Ignition 1 Voltage
4 | WH/BK | -- | Ignition Key Resistor Signal
5 | WH | -- | Off/Run/ Crank Voltage
6 | -- | -- | Not Used