For 1990-2009 cars

## Liftgate Outside Handle Replacement C100/Long Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the liftgate lower trim. Refer to Liftgate Trim Panel Replacement.
3. Disconnect the electrical connector.
4. Remove the nuts and the liftgate outside handle.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the liftgate outside handle with the nuts and tighten to 3 N·m (27 lb in).
2. Connect the electrical connector.
3. Remove the liftgate lower trim. Refer to Liftgate Trim Panel Replacement.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.

## Liftgate Outside Handle Replacement C105/Short Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the liftgate lower trim. Refer to Liftgate Trim Panel Replacement.
3. Disconnect the electrical connector.
4. Remove the nuts and the liftgate outside handle.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the liftgate outside handle with the nuts and tighten to 3 N·m (27 lb in).
2. Connect the electrical connector.
3. Install the liftgate lower trim. Refer to Liftgate Trim Panel Replacement.
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.