For 1990-2009 cars

## Headlining Trim Panel Replacement C100/Long Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the sunroof molding, if equipped.
3. Remove the passenger assist handles. Refer to Assist Handle Replacement .
4. Remove the plastic retaining clips in the headliner on the driver’s side.
5. Remove the sun visors. Refer to Sunshade Replacement .
6. Remove the power sunroof control switch, if equipped. Refer to Sunroof Switch Replacement .
7. Remove the windshield garnish molding. Refer to Windshield Garnish Molding Replacement .
8. Remove the center pillar upper garnish molding. Refer to Center Pillar Upper Garnish Molding Replacement .
9. Remove the quarter window garnish molding. Refer to Body Side Window Rear Garnish Molding Replacement .
10. Remove the plastic retainers in the headliner.
11. Recline both front seats.
12. Remove the headliner through a rear door.

### Installation Procedure

1. Recline both front seats.
2. Insert the headliner through a rear door.
3. Install the headliner behind the seats around the doors.
4. Install the plastic retainers.
5. Install the windshield garnish molding. Refer to Windshield Garnish Molding Replacement .
6. Instal the center pillar upper garnish molding. Refer to Center Pillar Upper Garnish Molding Replacement .
7. Install the quarter window garnish molding. Refer to Body Side Window Rear Garnish Molding Replacement .
8. Install the power sunroof control switch, if equipped. Refer to Sunroof Switch Replacement .
9. Install the sun visors. Refer to Sunshade Replacement .
10. Install the plastic retainers in the headliner on the driver’s side.
11. Install the passenger assist handles. Refer to Assist Handle Replacement .
12. Install the sunroof molding, if equipped.
13. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .

## Headlining Trim Panel Replacement C105/Short Body

### Removal Procedure

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the sunroof molding, if equipped.
3. Remove the passenger assist handles. Refer to Assist Handle Replacement .
4. Remove the dome lamp. Refer to Dome Lamp Replacement .
5. Remove the sun visors. Refer to Sunshade Replacement .
6. Remove the power sunroof control switch, if equipped. Refer to Sunroof Switch Replacement .
7. Remove the windshield garnish molding. Refer to Windshield Garnish Molding Replacement .
8. Remove the center pillar upper garnish molding. Refer to Center Pillar Upper Garnish Molding Replacement .
9. Remove the quarter window garnish molding. Refer to Body Side Window Rear Garnish Molding Replacement .
10. Remove the plastic retainers in the headliner.
11. Recline both front seats.
12. Remove the headliner through a rear door.

### Installation Procedure

1. Recline both front seats.
2. Insert the headliner through a rear door.
3. Install the headliner behind the seats around the doors.
4. Install the plastic retainers.
5. Install the windshield garnish molding. Refer to Windshield Garnish Molding Replacement .
6. Instal the center pillar upper garnish molding. Refer to Center Pillar Upper Garnish Molding Replacement .
7. Install the quarter window garnish molding. Refer to Body Side Window Rear Garnish Molding Replacement .
8. Install the power sunroof control switch, if equipped. Refer to Sunroof Switch Replacement .
9. Install the sun visors. Refer to Sunshade Replacement .
10. Install the dome lamp. Refer to Dome Lamp Replacement .
11. Install the plastic retainers in the headliner on the driver’s side.
12. Install the passenger assist handles. Refer to Assist Handle Replacement .
13. Install the sunroof molding, if equipped.
14. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .