For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

Note: Only lift the engine far enough to take the weight off the transaxle rear mount assembly.

1. Support the engine assembly using DW-110-060 fixture .
2. Remove the transaxle rear mount-to-bracket through bolt and nut.
3. Remove the transaxle rear mount bracket bolts from the transaxle.
4. Remove the transaxle rear mount bracket.
5. Remove the transaxle rear mount retaining bolts from the cradle.
6. Remove the transaxle rear mount.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the transaxle rear mount to the cradle and tighten bolts to 90 N·m (66 lb ft).

Note: Before tightening the transaxle front mount through bolt and nut, swing the engine assembly backwards and forwards or from the side to side for the proper alignment.

2. Install the transaxle rear mount bracket to the transaxle and tighten bolts to 90 N·m (66 lb ft).
3. Install the transaxle rear mount through bolt and nut and tighten to 90 N·m (66 lb ft).