For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the outside rearview mirror glass. Refer to Outside Rearview Mirror Glass Replacement .
3. Remove the screws and the side turn signal lamp assembly.
4. Disconnect the electrical connector.

### Installation Procedure

Important: The side turn signal lamp assembly has no serviceable items. LED’s are used to provide illumination. If any LED fails to function, the side turn signal lamp assembly must be replaced.

1. Connect the electrical connector.
2. Install the side turn signal lamp assembly with the screws.
3. Install the outside rearview mirror glass. Refer to Outside Rearview Mirror Glass Replacement .
4. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .