For 1990-2009 cars

#### Special Tools

J 28585 Snap Ring Remover

1. Install the front internal gear thrust washer race (530) on top of the output gear assembly.
2. Install the front internal gear thrust bearing assembly (519) on top of the front internal gear thrust washer race (530).

Important: The front internal gear (526) should turn freely counterclockwise, and should lock clockwise.

3. Install the front internal gear and overrun roller clutch assembly (526).

Important:

• | The apply plate (515) is 2.5 mm (0.100 in) thick.

• | The steel plates (517) are 1.95 mm (0.077 in) thick.

• | The backing plate (520) IS 3.8 mm (0.150 in) thick.

4. Install the low and reverse clutch apply plate (515)
5. Install the 4 steel plates (517) and the 5 fiber plates (516).
6. Install the low and reverse clutch backing plate (520).
7. Using J 28585 install the low and reverse clutch plate retaining ring (518), aligning the openings of the retaining ring towards the dowel pin in the case. Both ends of the retaining ring lock in the lug.