For 1990-2009 cars

Checks | Causes
--- | ---
3-5 Reverse Clutch Assembly |

• | Inspect for damaged splines or improper surface finish on 3-5 Reverse Clutch Plates (507-509), Backing Plate (510)

• | Inspect for damaged, worn or leaking 3-5 Reverse Clutch Piston Seals (504-506)

• | Inspect for warped 3-5 Rev/4-5-6 Clutch Housing (516)

• | Inspect for broken or fatigued 3-5 Reverse Clutch Waved Plate (507)