For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement.
2. Remove the driver information center bezel. Refer to Driver Information Display Bezel Replacement.
3. Remove the screws and the instrument panel lower compartment.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the instrument lower compartment with the screws and tighten to 2 N·m (18 lb in).
2. Install the instrument panel driver information center bezel. Refer to Driver Information Display Bezel Replacement.
3. Install the instrument panel center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement.