For 1990-2009 cars

### Removal Procedure

Important: Left - Hand Drive Shown, Right - Hand Drive Similar.

1. Remove the instrument panel lower left trim. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side .
2. Remove the screws and bolts.
3. Remove the driver knee bolster.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the driver knee bolster with the screws and bolts.

Tighten

• | Tighten the driver knee bolster screws to 2.5 N·m (23 lb in).

• | Tighten the driver knee bolster bolts to 20 N·m (15 lb ft).

2. Install the instrument panel lower left trim. Refer to Instrument Panel Lower Trim Panel Replacement - Left Side .