For 1990-2009 cars

#### Tools Required

J 36346 Fascia Retainer Remover

### Removal Procedure

1. Disable the SIR system. Refer to SIR Disabling and Enabling .
2. Remove the console. Refer to Console Replacement .
3. Using the J 36346 , disconnect the shift control cable from the shift control range select lever pin.
4. Squeeze the tabs on the shift control cable retainer clip and remove the cable from the shift control.
5. Squeeze the tabs on the park lock cable clip and pull upward to remove the cable from the shift control.
6. Disconnect the park lock cable from the shift control park lock lever.
7. Disconnect the shift control electrical connector.
8. Remove the nuts from the shift control.
9. Remove the shift control from the shift control mounting bracket.

### Installation Procedure

1. Install the shift control to the shift control mounting bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the shift control nuts.

Tighten
Tighten the nuts to 25 N·m (18 lb ft).

3. Connect the shift control electrical connector.
4. Install the park lock cable onto the shift control.
5. Install the park lock cable end terminal onto the park lock lever by aligning the cable fitting to the park lock lever pin and pushing forward. When installing, be sure not to install the cable end fitting on an angle or push down on the cable portion as this may cause cable to misadjust.
6. If the park lock cable becomes misadjusted. Refer to Park Lock Cable Replacement for the park lock cable adjustment procedure.
7. Install the shift control cable onto the shift control.
8. Connect the shift control cable onto the shift control range select lever pin.
9. Install the console. Refer to Console Replacement .
10. Enable SIR system. Refer to SIR Disabling and Enabling .